Those Verilog files are needed in order to perform the CPA measurements. Add (and replace if needed) those files to the AES Verilog files.